**General Features**

* Easy to use, oversized, full-color LCD touch panel display
* Delivers superior color output resolution up to 1200 x 1200 dpi
* Uses less power without changing workflow or inconveniencing users.
* One of the lowest Typical Electricity Consumption (TEC) values in the industry
* Standard DataOverwriteSecurity System automatically overwrites the HDD after each job
* Standard HDD Encryption encodes stored files for maximum defense against hackers
* Paper supply up to 4,400 sheets
* Delivers fast first copy in just 5.9 seconds (FC) or 3.7 seconds (B+W)
* Easy-to-replace toner cartridge
* Easy-to-grip paper tray handles
* Choose from a variety of professional finishing options including hole-punched, saddle-stitch and folded booklets
* Provides an array of document management capabilities including, but not limited to, archiving, managing, and sending/receiving files
* Multiple security levels both standard and optional to satisfy your security requirements
* Store and retrieve documents on-site with built-in Document Server
* View job queues and check supply levels with Web Image Monitor and SmartDeviceMonitor
* Print photos directly from a digital camera

**Copier Features**

* Scan once, print many
* Output speed of 45 ppm for full-color and black and white
* First Copy speed 5.9 seconds full-color, 3.7 seconds B+W
* Standard duplex with Automatic Reversing Document Feeder
* Max copy size 11” x 17”, full bleed on 12” x 18”
* Output onto letterhead, transparencies and special select stocks up to 12” X 18”

**Print Features**

* Output speed 45-ppm full color and black and white
* HotSpot MFP option lets mobile print users print directly from a laptop, handheld device or smart phone- including Blackberry® and iPhone® Standard interface 10BaseT/100BaseTX Ethernet (RJ-45), USB 2.0
* Full finishing capability with optional finishers
* Optional Fiery™ Controller (available Q1 2011) is ideal for users who require more sophisticated control over color workflows.

**Scanner Features**

* Scan-to-Email (with LDAP support), Scan-to-Folder, Scan-to-URL, and optional Scan to Media (USB/SD Card)
* Maximum scan size 11” x 17”